2024/08/09 21:15:44
================================================================
> Starfish v0.25
> 2D Plasma / Rarefied Gas Simulation Code
> (c) 2012-2024, Particle In Cell Consulting LLC
> info@particleincell.com, www.particleincell.com

!! This is a development version. The software is provided as-is, 
!! with no implied or expressed warranties. Report bugs to 
!! bugs@particleincell.com
=================================================================
Added interaction DSMC
Added interaction MCC
Added sigma BIRD463
Added solver BOYD
Added solver GENG
Added solver MAG
Added material type GRAIN
Added surface source DROPLET
Added material type SOLID
Added material type KINETIC
Added material type FLUID_DIFFUSION
Added material type BOLTZMANN_ELECTRONS
Added sigma CONST
Added sigma POLY
Added sigma INV
Added sigma LN
Added sigma TABLE
Added interaction SURFACE_HIT
Added interaction SURFACE_IMPACT
Added interaction CHEMISTRY
Added interaction ENERGY_TRANSFER
Added interaction SPUTTERING
Added interaction SURFACE_EMISSION
Added surface impact model NONE
Added surface impact model ABSORB
Added surface impact model SPECULAR
Added surface impact model DIFFUSE
Added surface impact model COSINE
Added sputtering model CONST
Added surface source UNIFORM
Added surface source MAXWELLIAN
Added surface source AMBIENT
Added surface source COSINE
Added surface source THERMIONIC
Added surface source VAPORIZATION
Added volume source PRELOAD
Added volume source MAXWELLIAN
Added solver CONSTANT-EF
Added solver QN
Added solver POISSON
Registered file reader type TECPLOT
Registered file reader type TABLE
Loading starfish.xml
Loading domain.xml
Loading materials.xml
Loading boundaries.xml
Loading interactions.xml
Processing <note>
**Starfish Tutorial: Part 6**
Processing <domain>
Domain type: XY
Added UNIFORM_MESH
> nodes   = 81 : 41
> origin  = -0.15 : 0.0
> spacing = 0.005 : 0.005
Processing <materials>
Added KINETIC material 'O+'
> charge   = 1.60217646E-19
> mass = 2.657e-26 (kg)
> spwt = 1000.0
Added KINETIC material 'iO+'
> charge   = 0.0
> mass = 2.657e-26 (kg)
> spwt = 1000.0
Added KINETIC material 'O'
> charge   = 0.0
> mass = 2.657e-26 (kg)
> spwt = 500.0
Added SOLID material 'SS'
Processing <boundaries>
Added solid boundary 'cylinder'
Added virtual boundary 'inlet'
Processing <material_interactions>
Added SURFACE_IMPACT O+ + SS -> O
> probability   = 0.9
> restitution  = 0.9
> thermal accomodation = 0.5
